================================================
FTDXCAT & SPLITTER – NEW INSTALLATION PROCEDURE
(c) 2020-2025 by HB9OAB (hb9oab@gmail.com)
================================================

Application for Yaesu FTDX101MP, FTDX101D, FTDX10, FT-710, FT-991/FT-991A, and now also for FTX-1.

⇒ Unzip the package into a folder, then simply run the <.exe> installer.
The new installation will automatically overwrite and remove the previous version.

IMPORTANT

If you previously installed the application using the old procedure, you may see two versions listed:

FTDX101 (old)

FTDX101CATsplitter (new)

If you encounter any issues, follow these FAQs:

UNINSTALL the OLD APP using the standard Windows uninstall procedure.
(If you are installing a newer version, uninstalling is not required — only do this if you want to reinstall the same version.
For safety, however, uninstalling is always recommended.
Your saved configuration and registration information will NOT be deleted.)

UNZIP the complete FTDX101 directory.

INSTALL the NEW RELEASE by running <setup.exe>.

REGISTER the newly installed application (*).

NOTE (*)

Starting from v1.5, your license key and personal configuration remain active on your PC even after uninstalling, reinstalling, or updating the application.

ATTENTION

If you experience installation problems, please carefully read the FAQ published here:
http://radioclub.ddns.net/ftdx101cat/faq.htm

Please read the News, Information, and Update History here:
http://radioclub.ddns.net/ftdx101cat/history.htm

Register your application using your personal serial code:
MENU → INFO → REGISTER

Main page:
http://radioclub.ddns.net/ftdx101

NOTICE

For Yaesu monitors without SCULAN10, please read history.txt in the FTDX101CAT & SPLITTER menu.

Full README, NEWS, and HISTORY:
http://radioclub.ddns.net/ftdx101cat/history.htm